Neb example
-------------

Once the env.sh file in the i-pi root directory has been sourced with

```bash
source <i-pi-root>/env.sh
```

Run i-pi with:

```bash
i-pi input.xml
```

And the driver:

```bash
i-pi-driver -u -h driver -p 20614 -m zundel
```
