### ground truth

To set your Viomi water heater to work in a specific mode and schedule it to run at a specific time, follow these steps:
1. Press the '电源' button (with the power symbol) to turn on the water heater if it is currently off.
2. Press the '模式调节' button (labeled with '模式调节') to adjust and select the desired mode. Press this button multiple times, if necessary, until you reach the required mode.
3. Press the '预约' button (labeled with '预约') to initiate the reservation setting function. This will prepare the water heater to accept the reservation settings.
4. Use the 'left arrow' button (icon of a left arrow) and the 'right arrow' button (icon of a right arrow) to navigate and set the reservation time accordingly.
5. Confirm the reservation if needed by pressing any additional buttons as per the water heater's interface instructions.

### question

You want to set your Viomi water heater to work in a specific mode and schedule it to run at a specific time. How would you go about setting the mode and making a reservation?

### prediction of yi-7b-ft

To set the Viomi water heater to a specific mode and schedule its operation, follow these steps:
1. Press the '电源' button (with the power symbol) to turn on the water heater if it is currently off. This will power up the water heater.
2. Press the '模式' button (with the light bulb and checkmark icon) to select or confirm the desired working mode of the water heater. Continue pressing until the desired mode is indicated.
3. Press the '预约' button (with the clock icon) to enter the reservation mode. This will allow you to set the specific time for the water heater to start.
4. Use the 'right arrow' button (with the right arrow icon) to confirm and set the reservation time. Pressing this button will finalize the chosen time for the water heater to begin heating.

### LLM-as-Judge

The plan is 0 because the second process omits the use of the 'left arrow' button to navigate and set the reservation time, and it also lacks confirmation of the reservation by pressing any necessary additional buttons.