### Question

- A button from (0.425, 0.69) to (0.495, 0.729).
- A button from (0.313, 0.688) to (0.387, 0.73).
- A button from (0.422, 0.473) to (0.508, 0.535).
- A button from (0.312, 0.764) to (0.385, 0.809).
- A button from (0.316, 0.613) to (0.402, 0.679).
- A button from (0.531, 0.763) to (0.602, 0.805).
- A button from (0.419, 0.524) to (0.507, 0.587).
- A button from (0.328, 0.501) to (0.383, 0.578).
- A button from (0.533, 0.688) to (0.601, 0.729).
- A button from (0.423, 0.764) to (0.493, 0.806).
- A button from (0.53, 0.418) to (0.606, 0.496).
- A button from (0.534, 0.613) to (0.606, 0.653).
- A button from (0.532, 0.503) to (0.596, 0.58).
- A button from (0.32, 0.413) to (0.39, 0.493).
- A button from (0.414, 0.613) to (0.499, 0.679).

### System Prompt

This image captures a panel of an appliance in real world. I will give you the type and location information of every module on this panel, you should enrich every module information by appending its description and function. Retain the original type and information details, following the original order and section format.

### Prediction

- A button from (0.425, 0.69) to (0.495, 0.729). It has 'TIME OFF' on it and looks like . This is a button. Its possible function is to set the air conditioner to turn off at a scheduled time. After pressing it, the air conditioner can stop running after the set time. .
- A button from (0.313, 0.688) to (0.387, 0.73). It has 'TIME ON' on it and looks like . This is a button. Its possible function is to set the scheduled start time of the air conditioner. After pressing it, the air conditioner can be started and run according to the set time. .
- A button from (0.422, 0.473) to (0.508, 0.535). It has 'TEMP' on it and looks like An arrow pointing up. This is a button which may be used to adjust the temperature. When pressed, it may increase the set temperature of the air conditioner. .
- A button from (0.312, 0.764) to (0.385, 0.809). It has 'Set' on it and looks like A blue button with the word 'Set'. This is a blue button labeled "Set". Its possible function is to perform the setting operation of the air conditioner. After pressing it, relevant parameters of the air conditioner can be set. .
- A button from (0.316, 0.613) to (0.402, 0.679). It has 'A.SWING' on it and looks like . This is a button, which may be used to control the automatic swing function of the air conditioner. Pressing it may turn on or off the automatic swing mode. .
- A button from (0.531, 0.763) to (0.602, 0.805). It has 'OK' on it and looks like . This is a button. Its possible function is to confirm an operation. After pressing it, a certain setting of the air conditioner can be confirmed or an operation can be executed. .
- A button from (0.419, 0.524) to (0.507, 0.587). It has 'TEMP' on it and looks like triangle pointing down. This is a button which may be used to adjust the temperature. When pressed, it may lower the set temperature of the air conditioner. .
- A button from (0.328, 0.501) to (0.383, 0.578). It has 'MODE' on it and looks like . This is a button. Its possible function is to switch the air conditioner mode. After pressing it, the air conditioner can be switched between different operating modes (such as cooling, heating, dehumidifying, air supply, etc.). .
- A button from (0.533, 0.688) to (0.601, 0.729). It has 'E-heat' on it and looks like . This is a button. Its possible function is to turn on the electric auxiliary heating. After pressing it, the electric auxiliary heating function of the air conditioner can be started. .
- A button from (0.423, 0.764) to (0.493, 0.806). It has 'CLOCK' on it and looks like A clock icon with two arrows forming a circular motion.. This is a button which may be used to adjust the clock settings of the air conditioner. Pressing it may start or confirm the time adjustment. .
- A button from (0.53, 0.418) to (0.606, 0.496). It has 'ON/OFF' on it and looks like A power symbol, typically used to indicate the on/off function.. This is a button. Its possible function is to control the turning on and off of the air conditioner. Pressing it can turn the air conditioner on or off. .
- A button from (0.534, 0.613) to (0.606, 0.653). It has 'F.Cool' on it and looks like . This is a button. Its possible function is to provide rapid cooling. When pressed, the air conditioner will immediately operate at its maximum cooling capacity. .
- A button from (0.532, 0.503) to (0.596, 0.58). It has 'WIND' on it and looks like A symbol representing wind, typically a spiral or swirl icon.. This is a button. Its possible function is to control the air outlet mode of the air conditioner. After pressing it, different air outlet modes can be switched (such as natural wind, circulating wind, etc., with different modes represented by spiral or vortex icons). .
- A button from (0.32, 0.413) to (0.39, 0.493). It has 'LIGHT' on it and looks like A yellow button with a lightbulb icon, representing the light function.. This is a yellow button marked "LIGHT". Its possible function is to control the lights of the air conditioner. Pressing it can turn on or off the lights of the air conditioner. .
- A button from (0.414, 0.613) to (0.499, 0.679). It has 'M.Swing' on it and looks like four arrows pointing to left-bottom. This is a button that may be used to manually control the function of the air conditioner's air direction swing. When pressed, it will start or stop the automatic swing of the air direction. .