### Question

- A button from (0.562, 0.375) to (0.678, 0.441).
- A button from (0.311, 0.15) to (0.433, 0.219).
- A button from (0.514, 0.239) to (0.644, 0.308).
- A button from (0.504, 0.179) to (0.621, 0.24).
- A button from (0.546, 0.31) to (0.661, 0.374).
- A button from (0.503, 0.144) to (0.618, 0.205).
- A button from (0.37, 0.35) to (0.482, 0.416).
- A button from (0.354, 0.281) to (0.463, 0.35).
- A button from (0.42, 0.554) to (0.518, 0.644).
- A button from (0.606, 0.536) to (0.717, 0.619).
- A button from (0.331, 0.214) to (0.449, 0.286).
- A button from (0.4, 0.48) to (0.515, 0.548).

### System Prompt

This image captures a panel of an appliance in real world. I will give you the type and location information of every module on this panel, you should enrich every module information by appending its description and function. Retain the original type and information details, following the original order and section format.

### Prediction

- A button from (0.562, 0.375) to (0.678, 0.441). It has 'Timer' on it and looks like . This is a button. Its possible function is to set the timer function of the air conditioner. After pressing it, you can set the duration for the air conditioner to turn on or off at a scheduled time. .
- A button from (0.311, 0.15) to (0.433, 0.219). It has 'Fan Slower' on it and looks like . This is a button. Its possible function is to reduce the speed of the air conditioner fan. Pressing it can make the rotational speed of the air conditioner fan become slower. .
- A button from (0.514, 0.239) to (0.644, 0.308). It has 'Energy Saver' on it and looks like . This is a button. Its possible function is to turn on the energy-saving mode of the air conditioner. After pressing it, the energy consumption of the air conditioner can be reduced. .
- A button from (0.504, 0.179) to (0.621, 0.24). It has 'Temp/Timer' on it and looks like reduce. This is a button that may be used to decrease the temperature or the timing duration. When pressed, it may lower the currently set temperature or reduce the remaining time of the timer. .
- A button from (0.546, 0.31) to (0.661, 0.374). It has 'Sleep' on it and looks like . This is a button. Its possible function is to turn on the sleep mode of the air conditioner. After pressing it, the operating state of the air conditioner can be adjusted to adapt to the sleep environment. .
- A button from (0.503, 0.144) to (0.618, 0.205). It has 'Temp/Timer' on it and looks like up. This is a button that may be used to adjust the temperature or set a timer. When pressed, it may switch or increase the temperature or the timing duration. .
- A button from (0.37, 0.35) to (0.482, 0.416). It has 'Heat' on it and looks like . This is a button. Its possible function is to turn on the heating mode of the air conditioner. After pressing it, the air conditioner can enter the heating state. .
- A button from (0.354, 0.281) to (0.463, 0.35). It has 'Cool' on it and looks like . This is a button. Its possible function is to turn on the cooling mode of the air conditioner. Pressing it can make the air conditioner enter the cooling state. .
- A button from (0.42, 0.554) to (0.518, 0.644). It has 'Auto Fan' on it and looks like . This is a button. Its possible function is to control the automatic fan mode of the air conditioner. Pressing it can turn on or off the automatic fan function. .
- A button from (0.606, 0.536) to (0.717, 0.619). It has '' on it and looks like A power icon. This is a button, which may be used to control the power switch of the air conditioner. Pressing it may turn the air conditioner on or off. .
- A button from (0.331, 0.214) to (0.449, 0.286). It has 'Fan Faster' on it and looks like . This is a button. Its possible function is to increase the rotational speed of the air conditioner fan. After pressing it, the operating speed of the air conditioner fan can be increased. .
- A button from (0.4, 0.48) to (0.515, 0.548). It has 'Fan Only' on it and looks like . This is a button. Its possible function is to turn on the air conditioner's only blowing mode. After pressing it, the air conditioner can operate only in the blowing state. .