### ground truth

To set your Viomi water heater to work in a specific mode and schedule it to run at a specific time, follow these steps:
1. Press the '电源' button (with the power symbol) to turn on the water heater if it is currently off.
2. Press the '模式调节' button (labeled with '模式调节') to adjust and select the desired mode. Press this button multiple times, if necessary, until you reach the required mode.
3. Press the '预约' button (labeled with '预约') to initiate the reservation setting function. This will prepare the water heater to accept the reservation settings.
4. Use the 'left arrow' button (icon of a left arrow) and the 'right arrow' button (icon of a right arrow) to navigate and set the reservation time accordingly.
5. Confirm the reservation if needed by pressing any additional buttons as per the water heater's interface instructions.

### question

You want to set your Viomi water heater to work in a specific mode and schedule it to run at a specific time. How would you go about setting the mode and making a reservation?

### prediction of qwen-7b-ft_2

To set the Viomi water heater to work in a specific mode and schedule it to run at a specific time, follow these steps:
1. Press the '电源' button (with the power symbol) to turn on the water heater if it is currently off. This will power up the water heater and prepare it for operation.
2. Press the '模式' button (labeled with '模式') to select the desired working mode of the water heater. This will switch the heater to the appropriate mode as per your requirement.
3. Press the '预约' button (labeled with '预约') to set the reservation function. This will allow you to schedule the water heater to start working at a specific time.
4. Use the 'right arrow' button (with the right arrow icon) to confirm your settings and initiate the reservation. This will finalize the scheduled start time for the water heater.

### LLM-as-Judge

The plan is 0. The second sequence omits the use of the 'left arrow' button to navigate the reservation time, which deviates significantly from the first sequence, where both 'left arrow' and 'right arrow' buttons are required to set the reservation time accordingly.