### Question

- A button from (0.465, 0.41) to (0.6, 0.458).
- A button from (0.552, 0.413) to (0.682, 0.458).
- A button from (0.58, 0.612) to (0.638, 0.666).
- A button from (0.463, 0.528) to (0.513, 0.565).
- A button from (0.542, 0.529) to (0.605, 0.567).
- A button from (0.625, 0.575) to (0.703, 0.613).
- A button from (0.628, 0.53) to (0.699, 0.568).
- A button from (0.625, 0.481) to (0.687, 0.52).
- A button from (0.444, 0.611) to (0.518, 0.665).
- A button from (0.648, 0.625) to (0.699, 0.667).
- A button from (0.465, 0.481) to (0.511, 0.517).
- A button from (0.525, 0.476) to (0.623, 0.524).

### System Prompt

This image captures a panel of an appliance in real world. I will give you the type and location information of every module on this panel, you should enrich every module information by appending its description and function. Retain the original type and information details, following the original order and section format.

### Prediction

- A button from (0.465, 0.41) to (0.6, 0.458). It has 'TEMP' on it and looks like . This is a button. Its possible function is to adjust the air-conditioning temperature. After pressing it, relevant operations can be performed on the air-conditioning temperature. .
- A button from (0.552, 0.413) to (0.682, 0.458). It has 'TEMP' on it and looks like . This is a button. Its possible function is to adjust the air-conditioning temperature. After pressing it, the set temperature of the air conditioner can be adjusted. .
- A button from (0.58, 0.612) to (0.638, 0.666). It has 'LED DISPLAY' on it and looks like . This is a button. Its possible function is to control the LED display screen of the air conditioner. After pressing it, relevant operations can be performed on the display screen (such as turning the display screen on/off, switching the display mode, etc.). .
- A button from (0.463, 0.528) to (0.513, 0.565). It has 'SWING' on it and looks like . This is a button, which may be used to control the air swing function of the air conditioner. After pressing it, the air direction of the air conditioner will start to swing up and down or left and right. .
- A button from (0.542, 0.529) to (0.605, 0.567). It has 'SLEEP' on it and looks like . This is a button. Its possible function is to turn on the sleep mode of the air conditioner. After pressing it, the air conditioner can enter an operating state suitable for sleep. .
- A button from (0.625, 0.575) to (0.703, 0.613). It has 'TIMER OFF' on it and looks like . This is a button. Its possible function is to turn off the air conditioner timer. Pressing it can turn off the timing function of the air conditioner. .
- A button from (0.628, 0.53) to (0.699, 0.568). It has 'TIMER ON' on it and looks like . This is a button. Its possible function is to turn on the air conditioner timer. After pressing it, you can set the air conditioner to run at a scheduled time. .
- A button from (0.625, 0.481) to (0.687, 0.52). It has 'FAN SPEED' on it and looks like . This is a button. Its possible function is to adjust the air conditioner fan speed. After pressing it, different fan speed gears can be switched. .
- A button from (0.444, 0.611) to (0.518, 0.665). It has 'AIR DIRECTION' on it and looks like . This is a button. Its possible function is to adjust the air outlet direction of the air conditioner. After pressing it, the angle of the air outlet of the air conditioner can be changed. .
- A button from (0.648, 0.625) to (0.699, 0.667). It has 'TURBO' on it and looks like . This is a button. Its possible function is to turn on the strong mode of the air conditioner. After pressing it, the air conditioner can operate at a stronger power. .
- A button from (0.465, 0.481) to (0.511, 0.517). It has 'MODE' on it and looks like . This is a button. Its possible function is to switch the air conditioner mode. After pressing it, it can be switched between different operating modes (such as cooling, heating, dehumidifying, air supply, etc.). .
- A button from (0.525, 0.476) to (0.623, 0.524). It has 'ON/OFF' on it and looks like . This is a button. Its possible function is to control the turning on and off of the air conditioner. Pressing it can achieve the operation of turning on or off the air conditioner. .